**Features and benefits of the Cordless Torque Multiplier include:**

* 3/4” drive size: CTM600SS; 118 – 600 ft-lb torque range
* 1” drive size available in three torque range options
	+ CTM1000: 250 – 1,000 ft-lb
	+ CTM2000: 500 – 2,000 ft-lb
	+ CTM3000: 750 – 3,000 ft-lb
* Cordless design where a hose-free workplace would be safer, or in the field where access to power is unavailable
* Brushless motor eliminates need for tool to stop and cool down, increasing runtime and productivity
* Multiple units of torque measurement, including N•m and ft-lb
* Torque, torque and angle with final torque and torque audit functionality available in “advanced” mode
* Clear indication of successful joint application
* User-specific functionality
	+ 12 user IDs can be downloaded to the tool and results can be stored against individual users
	+ 20 unique stand-alone targets, plus 20 unique work group targets for each work group
	+ Maximum audit mode target angle (720°)
* 1" square drive is quickly and easily replaceable
* Safe-to-start button to promote safe hand positioning at start up
* Handle and trigger designed for optimum comfort
* Key lock prevents unauthorized usage
* 18 V, 5.0Ah battery and efficient motor give outstanding fastening performance per charge